SPRAYON PRODUCTS (PTY) LTD

MATERIAL SAFETY DATA SHEET

Date issued 01/02/2018
BC1 : BURNISHING COMPOUND                 DNM

SECTION 1. PRODUCT AND COMPANY IDENTIFICATION 

Product Code 	BC1	Product Name 	BURNISHING COMPOUND                DNM 
CAS No. 	Not applicable 	EC No 	Not applicable 	UN No 	1263

Company Name 	Sprayon Products
			222 2nd Street
			Wynberg

Emergency contact no: 011-440-2202

SECTION 2. COMPOSITION/INFORMATION ON INGREDIENTS 

Chemical Class 	PAINT or PAINT RELATED
Classification 	- Xn    R Phrases R10,65,36/38   S Phrases S02,13,26,43A,62
Comment 	 OEL Type : Mixture - See tables in Sections 2 and 8 

 	% m/m 	EC Labels 	CAS No. 	EC No.
HAZARDOUS AND/OR OTHER RELEVANT COMPONENTS
WHITE SPIRIT  (WS3) 	<41 % 	Xn 	64742-88-7 	649-405-00-X
TETRAHYDRO-1,4-OXAZINE, MORPHOLINE 	<2 % 	C 	110-91-8 	613-028-00-9

SECTION 3. HAZARDS IDENTIFICATION 

SAPMA Health Rating 	 2-MODERATE - Temporary or minor injury possible even if treatment given
Inhalation 	Irritating.
Skin 	Highly irritating.  Risk of dermatitis.  May be absorbed through intact skin.
Eyes 	Irritating - may cause damage if not given prompt attention.
Ingestion 	Harmful.  May cause lung damage if swallowed.
No carcinogenic, mutagenic or genetic effects established
May have short term environmental effects. Contain, monitor & remove

SECTION 4. FIRST AID MEASURES 

Inhalation 	Move to fresh air.
Skin 	Drench with water. Remove contaminated clothing. Use a skin cleaner. In severe cases refer to Doctor.
Eyes 	Rinse well with water and seek medical advice if discomfort persists.
Ingestion 	DO NOT INDUCE VOMITING.  Get immediate medical attention.

SECTION 5. FIRE FIGHTING MEASURES 

Flammable with toxic fumes. 
Containers liable to burst in a fire. 
Foam. CO2. Dry powder. Fog to cool and control. Do NOT use water jets. 

SECTION 6. ACCIDENTAL RELEASE MEASURES - SEE ALSO SECTIONS 5, 8, 13 

Contain & collect.  Keep out of drains and sewers

SECTION 7. HANDLING AND STORAGE 

Store separately from any reactive substances - oxidisers in particular. 
No open flames. No smoking. 
Store containers with due care in case of fire. 
Subject to local bylaws 

SECTION 8. EXPOSURE CONTROLS/PERSONAL PROTECTION 
  
	 	  CAS No. 	  OEL 	  OEL 	  STOEL 	  STOEL 	  OEL 
	 	   	  (mg/m3) 	  (ppm) 	  (mg/m3) 	  (PPM) 	  Type 
	HAZARDOUS AND/OR OTHER RELEVANT COMPONENTS 

	WHITE SPIRIT  (WS3) 	 64742-88-7 	 575 	 100 	 720 	 125 	 RL 
	TETRAHYDRO-1,4-OXAZINE, MORPHOLINE 	 110-91-8 	 71.0 	 20.0 	  	  	 RL S 
		(CL/RL = Controlled/Recommended level   'S' = Skin annotation) 

SAPMA Rating 	2-H-E PPE : Respirator and Eye protection 
Inhalation 	In case of insufficient ventilation, use suitable respiratory protection. 
Skin 	AVOID CONTACT.  Use impervious gloves, apron and boots. 
Eyes 	Avoid any form of direct contact. Do not touch eyes with dirty hands or gloves. 
Ingestion 	Observe the rules of hygiene. Wash before eating or drinking. 
 	 OEL Type : Mixture - See tables in Sections 2 and 8  

 

SECTION 9. PHYSICAL AND CHEMICAL PROPERTIES 

Appearance 	Water based dispersion 	Odour 	Typical
pH 	6-8 	Boiling Point 	>35°C
Flash Point 	>23°C   (derived) 	Water solubility 	 miscible

SECTION 10. STABILITY AND REACTIVITY 

Stable under normal conditions
No reaction with fire-fighting water

SECTION 11. TOXICOLOGICAL INFORMATION 

No carcinogenic, mutagenic or genetic effects established
LD50 Oral: >500 mg (derived)	

SECTION 12. ECOLOGICAL INFORMATION 

May have short term environmental effects. Contain, monitor & remove

SECTION 13. DISPOSAL INFORMATION 

Use reputable waste disposal contractors. Exercise caution in disposal of used containers.

SECTION 14. TRANSPORT INFORMATION 

UN Number 	1263
Shipping Name 	PAINT or PAINT RELATED MATERIAL
IMO Class 	3.3 	Packing Group 	III
Action Code 	127
HazChem 	3[Y]
Kemler Code 	30

SECTION 15. REGULATORY INFORMATION 

EC no. : n/a
- Xn    R Phrases R10,65,36/38   S Phrases S02,13,26,43A,62
R10 - Flammable
R65 - Harmful: May cause lung damage if swallowed.
R36/38 - Irritating to eyes and skin
S2 - Keep out of reach of children. (Retail sales items)
S13 - Keep away from food, drink and animal feeding stuffs
S26 - In case of contact with eyes, rinse immediately with plenty of water and seek medical advice
S43A - In case of fire, use water fog, foam or powder - Do not use water jets!
S62 - If swallowed, do not induce vomiting : seek medical advice immediately and show this container or label.

SECTION 16. OTHER INFORMATION 

TAKE PRECAUTIONARY MEASURES AGAINST STATIC DISCHARGES.
IN CASE OF ANY DISCOMFORT ALWAYS SEEK MEDICAL ADVICE.
	_ 

This MSDS conforms with General Administrative Regulations of 6 Sept.1996 (ISO-11014/ANSIZ400.1.1996) 
OELs derived from OHS Act Regulations for Dangerous Chemical Substances of 25 Aug.1995 (EH-42) 
SAPMA Rating - South African Paint Manufacturers Association Guide to Health Hazards (SABS ARP 006:1991) 
All information is given in good faith but without guarantee in respect of accuracy. 
No responsibility is accepted for errors or omissions or the consequences thereof. 
 
. 
Date: 01/02/2026

Rev:  2026A